
//============================================================================
//
//                   (C) COPYRIGHT 2001-2008 SYNOPSYS, INC.
//                            ALL RIGHTS RESERVED
//
// This software and the associated documentation are confidential and
// proprietary to Synopsys, Inc.  Your use or disclosure of this
// software is subject to the terms and conditions of a written
// license agreement between you, or your company, and Synopsys, Inc.
//
// The entire notice above must be reproduced on all authorized copies
//
// : //dwh/DW_ocb/DW_memctl/main/bin/ParamsParser.pl 
/ : #3 
/
// Abstract  : DW_memctl, synchronous write, and asynchronous read FIFO. 
// combinational flags and read-data.
//
//============================================================================
  # Power-on Reset Register Values For Your Configuration

  # The "initialize" bit-0 of SDRAM Control Register(SCTLR), on power-on
  # will be set to "1" and after auto initialization sequence completion
  # will get reset to 0"

  Relative Address 0x00: SCONR = 32'h1c3388
  Relative Address 0x04: STMG0R = 32'h19d9451
  Relative Address 0x08: STMG1R = 32'h70008
  Relative Address 0x0C: SCTLR = 32'h3009
  Relative Address 0x10: SREFR = 32'h410
  Relative Address 0x14: SCSLR0_LOW = 32'h80000000
  Relative Address 0x18: SCSLR1_LOW = 32'h10000000
  Relative Address 0x1C: SCSLR2_LOW = 32'h20000000
  Relative Address 0x20: SCSLR3_LOW = 32'h30000000
  Relative Address 0x24: SCSLR4_LOW = 32'h40000000
  Relative Address 0x28: SCSLR5_LOW = 32'h50000000
  Relative Address 0x2C: SCSLR6_LOW = 32'h60000000
  Relative Address 0x30: SCSLR7_LOW = 32'h70000000
  Relative Address 0x54: SMSKR0 = 32'h80c
  Relative Address 0x58: SMSKR1 = 32'h26
  Relative Address 0x5C: SMSKR2 = 32'h21
  Relative Address 0x60: SMSKR3 = 32'h441
  Relative Address 0x64: SMSKR4 = 32'h861
  Relative Address 0x68: SMSKR5 = 32'h401
  Relative Address 0x6C: SMSKR6 = 32'h401
  Relative Address 0x70: SMSKR7 = 32'h401
  Relative Address 0x74: CSALIAS0_LOW = 32'h80000000
  Relative Address 0x78: CSALIAS1_LOW = 32'h18000000
  Relative Address 0x84: CSREMAP0_LOW = 32'h80000000
  Relative Address 0x88: CSREMAP1_LOW = 32'h12000000
  Relative Address 0x94: SMTMGR_SET0 = 32'h10441
  Relative Address 0x98: SMTMGR_SET1 = 32'h7c4f5b
  Relative Address 0x9C: SMTMGR_SET2 = 32'h1c4f5b
  Relative Address 0xA0: FLASH_TRPDR = 32'hc8
  Relative Address 0xA4: SMCTLR = 32'h2480
  Relative Address 0xA8: SYNC_FLASH_OPCODE = 32'h0
  Relative Address 0xAC: ETN_MODE_REG = 32'h0
  Relative Address 0xB0: SFCONR = 32'h22d
  Relative Address 0xB4: SFCTLR = 32'h10
  Relative Address 0xB8: SFTMGR = 32'h252
